Inspection & Maintenance Log

Wet Detention Pond
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North East Wisconsin Stormwatar Consor




Inspection Year:
	     

	

	Name of Site: 
	     
	
	Address:
	     

	

	Inspector:
	     
	
	Company:
	     

	

	Municipality Contact:
	     
	
	Phone:
	     


* Facility owner responsible for inspecting, maintaining, and repairing facility components after major storm events (greater than ½”), annually at a minimum.  Check any deficiencies noted and comment for maintenance actions taken, date of repair, and any alerts.  Inspection items with no * should be completed by a qualified professional every five years (or more frequently if concerns are noted).
	Inspection Item
	Storm Date
	Storm Date
	Storm Date
	Maintenance Action
	Date

	Pond


Bank Erosion *


Debris / Trash Accumulation *


Visible pollution *


Abnormal water levels *


Sediment Accumulation *


Depressions, Whirlpools, Sinkholes 


	
	
	
	Repair/Restore

Clean up/Remove
Contact Municipality
Contact Municipality
Dredge
Contact Municipality

	

	Embankment
1.  Upstream Slope- Poor Grass Cover*
     Erosion or Slides *
     Trees/Brush Growing on Slopes *
     Deficient Riprap Protection *
     Animal Burrows *

     Depressions or Bulges

     Settlement

     Longitudinal Cracks

     Transverse Cracks


	
	
	
	Revegetate

Repair/Restore

Remove

Repair

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality


	


	Inspection Item
	Storm Date
	Storm Date
	Storm Date
	Maintenance Action
	Date

	2.
Crest – Settlement *

Misalignment

Cracking



	
	
	
	Contact Municipality

Contact Municipality

Contact Municipality


	

	3.  Downstream Slope - Poor Grass Cover *

Erosion or Slides *
   
Trees/Brush Growing on Slopes *
   
Animal Burrows *

   
Excessive or Cloudy Seepage *

  
Longitudinal Cracks

  
Transverse Cracks

  
Depressions or Bulges

   
Settlement

  
Seeps, leaks, or boils


	
	
	
	Revegetate
Repair/Restore

Remove

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality


	

	4.
Emergency Spillway – Exposed Fabric *
    Overgrown Vegetation *
    Erosion/Backcutting at berm or road* 

    Rutting or pot-holes *
    Obstructions or debris *
    Inadequate Riprap/Armor *

    Cracking


Slumping/Sloughing of Embankment

Settlement
	
	
	
	Repair
Cut / Trim

Repair (fill, armor)

Repair

Remove

Repair

Contact Municipality
Contact Municipality

Contact Municipality
	

	Spillway

1.  Eroding or Backcutting *
     Overgrown Vegetation *
     Obstructions with Debris *
     Excessive Siltation *
     Slumping/Sloughing


	
	
	
	Repair (fill, armor)

Cut / Trim

Clear / Remove

Remove (dredge)

Contact Municipality
	

	Control Structure

1.  Inlet - Debris in Conveyance Area *

     Erosion or Undercutting *

     Stop-log deterioration / leaking *

     Joint Separation

     Cracks in Concrete

     Deteriorated piping

     Displacement of Structure


	
	
	
	Clear / Remove

Repair (fill, armor)
Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality
	


	2.  Outlet - Erosion or Backcutting *
     Debris in Culvert or Trash Rack *
     Undermining/Scour *
     Inoperable control valve *
     Inoperable flap gate *
     Joint Separation 

     Cracks in Concrete

	
	
	
	Repair (fill, armor)
Clear / Remove

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality
	

	Downstream Area

1.  Erosion *
     Debris / Obstructions *

	
	
	
	Contact Municipality

Clear / Remove
	

	2.  Bridge / Culvert Problems
     Buildings Issues
     Foundation Concerns

	
	
	
	Contact Municipality
Contact Municipality

Contact Municipality
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