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North East Wisconsin Stormwatar Consor




Inspection & Maintenance Log

Infiltration Basin


	Inspection Year:
	     

	

	Name of Site: 
	     
	
	Address:
	     

	

	Inspector:
	     
	
	Company:
	     

	

	Municipality Contact:
	     
	
	Phone:
	     


* Facility owner responsible for inspecting, maintaining, and repairing facility components after major storm events (greater than ½”), annually at a minimum.  Check any deficiencies noted and comment for maintenance actions taken, date of repair, and any alerts.  Inspection items with no * should be completed by a qualified professional every five years (or more frequently if concerns are noted).

	Inspection Item
	Storm Date
	Storm Date
	Storm Date
	Maintenance Action
	Date

	Inlet

Bank Erosion *

Debris / Trash Accumulation *

Visible pollution (oil sheen, algae, etc) *

High water levels *

Sediment Accumulation *

Inlet Dispersion System Failure (causing undesirable concentrated inflow)* 


	
	
	
	Repair/Restore

Clean up/Remove

Contact Municipality

Contact Municipality

Remove

Repair/Reconstruct


	

	Basin

Debris / Trash Accumulation *

Visible pollution *

Poor Vegetative Cover*                                

Erosion or Depressions *

Trees/Brush Growing within Basin *

Long-term Standing Water (greater than 3 days after rain event)*

Animal Burrows *

Undesirable Vegetation


	
	
	
	Repair/Restore

Contact Municipality

Revegetate

Repair/Restore

Remove/Revegetate

Restore (remove soils to 3”, chisel plow, add topsoil & compost)

Contact Municipality

Contact Municipality
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