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North East Wisconsin Stormwatar Consor




Inspection & Maintenance Log

Bioretention & Rain Garden


	Inspection Year:
	     

	

	Name of Site: 
	     
	
	Address:
	     

	

	Inspector:
	     
	
	Company:
	     

	

	Municipality Contact:
	     
	
	Phone:
	     


* Facility owner responsible for inspecting, maintaining, and repairing facility components after major storm events (greater than ½”), annually at a minimum.  Check any deficiencies noted and comment for maintenance actions taken, date of repair, and any alerts.  Inspection items with no * should be completed by a qualified professional every five years (or more frequently if concerns are noted).

	Inspection Item
	Storm Date
	Storm Date
	Storm Date
	Maintenance Action
	Date

	Outlet/Standpipe
     Debris / Trash Accumulation *

     High water levels (near top of basin) *
	
	
	
	Clean up/Remove

Contact Municipality


	

	Emergency Spillway

    Erosion or Depressions *

    Missing Rock 
	
	
	
	Repair/Restore

Repair/Restore

	

	Basin

Debris / Trash Accumulation *

Visible pollution (oil sheen, algae, etc.) *

Wilting/Dying Plants *                                

Erosion or Depressions *

Long-term Standing Water (greater than 3 days after rain event)*

Poor vegetation density

Animal Burrows *

Undesirable/Invasive vegetation 
     Voids in mulch area
	
	
	
	Remove
Contact Municipality

Water and/or Replant per approved plan
Repair/Restore

Restore (remove mulch scarify soils around plants, add new mulch)

Replant per approved plan

Contact Municipality

Contact Municipality

Add mulch to depth of 3”
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