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Catch Basin / Proprietary Device
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	Inspection Year:
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	Name of Site: 
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	Address:
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	Inspector:
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	Company:
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	Municipality Contact:
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	Phone:
	[bookmark: Text7]     



* Facility owner responsible for inspecting, maintaining, and repairing facility components after major storm events (greater than ½”), annually at a minimum.  Check any deficiencies noted and comment for maintenance actions taken, date of repair, and any alerts.  Inspection items with no * should be completed by a qualified professional every five years (or more frequently if concerns are noted).

	Inspection Item
	Storm Date
	Storm Date
	Storm Date
	Maintenance Action
	Date

	Catch Basin / Proprietary Device

Inlet Protection *


Debris / Trash Accumulation *

Abnormal water levels *

Sediment / Floatables Accumulation *




Depressions around facility

Joint Separation

Cracks in Concrete

Deteriorated piping

Displacement of Structure
 

	
	
	
	

Remove after Stabilization

Clean up/Remove

Contact Municipality

Remove (pump and dispose of at wastewater treatment plant) **

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

Contact Municipality

	



** Pumping Details (based on design guidelines):

	Type of unit(s)
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	Design Pumping Frequency
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	Dates Pumped
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	Pumper
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	Disposal Location
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